EXTERIORGUARD® **OUTDOOR GUARDRAIL WORKSHEET**

Contact Name Company Address


Phone Fax Email Zip Code of Destination

**For a "Quick Quote" with freight charge**

**FAX TO: 724-446-0988**

DOUBLE RAIL CONFIGURATION

# 44” high, 42” to top of rail



Please sketch your layout below. Beside each rail, note dimension. Layout will be calculated with standard nominal rail lengths of 2, 3, 4, 5, 6, 7 or 8 feet. *Nominal rail length dimension is from center of post to center of post.* We will respond within one business day with job and freight pricing. If you need layout assistance, please call 1-800-868-5438.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

Exteriorguard® by Herwin Safety, Inc.

**1-800-868-5438 FAX : 724-446-0988** [**sales@herwin.biz**](mailto:sales@herwin.biz)

**2021 Herwin Safety, Inc. All rights reserved**