GUARDSMITH®

**For a "Quick Quote" with freight charge**

**FAX TO: 724-446-0988**

GUARDRAIL WORKSHEET

**RAIL CONFIGURATIONS *(please check)***

Double Rail (D)




44" high, 42" to top of rail

Single Rail (S)

18" high , 17" to top of rail

Lift-Out Brackets (U)

***For Interior Guardrail***

Contact Name Company Address

Phone Fax Email Zip Code of Destination

Please sketch your layout below. Beside each rail, note dimension and mark "D" for Double rail, "S" for Single rail, or "U" for Lift-Out bracket. Layout will be calculated with standard nominal rail lengths of 2, 3, 4, 5, 6, 7, 8, 9, or 10 feet. *Nominal rail length dimension is from center of post to center of post.* We will respond within one business day with job and freight pricing. If you need assistance with the layout, please call **1-800-868-5438**.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

Guardsmith® by Herwin Safety, Inc.

**CALL: 1-800-868-5438 FAX: 724-446-0988 EMAIL:** [**s**](mailto:sales@herwin.biz)[**ales@herwin.biz**](mailto:ales@herwin.biz)

**2021 Herwin Safety, Inc. All rights reserved**