NOTCHGUARD® **GUARDRAIL WORKSHEET**

**NOTCHGUARD® CONFIGURATIONS**

***(please check)***

Double Rail (D)

44" high, 42" to top of rail


Single Rail (S)


18" high, 12" to top of rail

Lift-Out Brackets (U)

**For a "Quick Quote" with freight charge**

**FAX TO: 724-446-0988**

Contact Name Company Address

Phone  Fax

Email Zip Code of Destination

Please sketch your layout below. Beside each rail, note dimension and mark "D" for Double rail, "S" for Single rail or "U" for Lift-Out bracket. Layout will be calculated with standard nominal rail lengths of 2, 3, 4, 5, 6, 7, 8, 9, or 10 feet. *Nominal rail length dimension is from center of post to center of post.* We will respond within one business day with job and freight pricing. If you need assistance with the layout, please call **1-800-868-5438**.

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

Notchguard® by Herwin Safety, Inc.

**1-800-868-5438 FAX: 724-446-0988** [**sales@herwin.biz**](mailto:sales@herwin.biz)

**2021 Herwin Safety, Inc. All rights reserved**